The encoder is the main input device for the handset. It is a 5-pin component. The side with 2 pins is the momentary switch, and the 3-pins are the encoder. The center pin on the encoder side is ground.