Notes for Platform I/O on Linux

To use the UBS-C port on the RISC-V MCU, Platform IO needs to have dfu-util installed.

[Index of /releases (sourceforge.net)](http://dfu-util.sourceforge.net/releases/)

Change platformio.ini, comment/uncomment your upload method:

upload\_protocol = dfu

; upload\_protocol = serial

; upload\_port = /dev/ttyUSB1

Linux users have to install [udev](https://en.wikipedia.org/wiki/Udev) rules for PlatformIO supported boards/devices. The latest version of rules may be found at <https://raw.githubusercontent.com/platformio/platformio-core/master/scripts/99-platformio-udev.rules>

[Frequently Asked Questions — PlatformIO 5.2.0a4 documentation](https://docs.platformio.org/en/latest/faq.html#platformio-udev-rules)

Comment out the following line in file:

-See “Using Platform I/O with RISC-V" in the notes folder.